{"text_format":"3","workbook":"xlsx","n_sheets":2,"sheets":["清单","计算式"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"清单","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"merged":[[0,0,0,6],[2,0,2,1],[3,1,5,1],[9,1,12,1],[13,1,15,1],[18,1,20,1],[26,1,27,1]]}
["淳安县第一人民医院功能提升改造项目(二期)院史陈列馆优化提升项目采购参数"]
["序号","展区","名称","规格型号","单位","数量","备注"]
["多媒体互动展项工程"]
[1,"党建","65寸触摸一体机","定制65触摸一体机\n1、屏幕比例：16:9；\n2、对比度：5000：1；\n3、响应时间：8ms\n4、分辨率：3840×2160；\n5、刷屏率：60Hz；\n6、支持来电自启；\n8、mini工控主板I5、 8G、 256G固态硬盘","台",1]
[2,null,"一体机安装支架-65寸","定制一体机安装支架，液压安装支架","套",1]
[3,null,"触摸软件","资料收集整理细化、风格设计/UI设计制作、唤醒触发及响应方式,设计制作、程序框架制作、触摸互动内容制作，不含音视频制作","套",1]
[4,"微观大冒险","信号放大器","显微镜信号传输器","套",1]
[5,"影像探秘空间","内容制作-影片剪辑","资料收集整理细化、创意策划及分镜头脚本、平面背景风格设计、过渡特效合成、渲染调色、素材包装剪辑输出、数字(视频/音频)内容合成，","秒",30]
[6,"细胞攻坚战","触摸互动软件（上下屏互动）","资料收集整理细化、风格设计/UI设计制作、唤醒触发及响应方式,设计制作、程序框架制作、触摸互动内容制作，不含音视频制作","套",1]
[7,"洗手观察站","32寸触摸一体机","定制32寸显示一体机\n1、屏幕比例：16:9；\n2、对比度：5000：1；\n3、响应时间：8ms\n4、分辨率：1920×1080；\n5、刷屏率：60Hz；\n6、支持来电自启；\n8、mini工控主板I5、 8G、 256G固态硬盘","台",1]
[8,null,"一体机安装支架-32寸","定制一体机安装支架，液压安装支架","套",1]
[9,null,"互动模块","1点感应模块及7点灯光控制模块","套",1]
[10,null,"互动控制软件","定制洗手互动软件：按照墙面七步洗手法完成动作，根据视频内容步骤，灯光同步点亮。","套",1]
[11,"医生训练营","32 寸触摸一体机","定制32 寸触摸一体机\n1 、屏幕比例：16:9；\n2 、对比度：5000：1；\n3 、响应时间：8ms\n4 、分辨率：1920×1080；\n5 、刷屏率：60Hz；\n6 、支持来电自启；\n8 、mini 工控主板 I5 、  8G 、  256G 固态硬盘","台",1]
[12,null,"互动模块","15点灯光控制模块","套",1]
[13,null,"互动控制软件","1、急救流程互动：点击屏幕模拟拨打电话，触发流程图灯光，声音同步播放急救指导。","套",1]
[14,"签名软件","签名软件（触摸端和显示端）","资料收集整理细化、风格设计/UI设计制作、唤醒触发及响应方式设计制作、程序框架制作、触摸签名软件制作，","套",1]
[15,"线材辅料","线材辅料","新的线路铺设，线材辅料","项",1]
[16,"基本做法：3D建模打印，内置互动灯光和配套控制","心脏信息互动模型","3D建模打印心脏模型，表面细节人工打磨、上色、内置流水灯带和配套控制器安装、仿心跳的震动，观察灯光沿心房、心室及血流路径依次亮起。","项",1]
[17,null,"肺部信息互动模型","3D建模打印肺部放大模型，表面细节人工打磨、上色、内置灯带和配套控制器安装，跟随提示深呼吸，观察支气管树灯光随呼吸节奏明暗变化。","项",1]
[18,null,"消化信息系统互动模型","3D建模打印消化系统模型，内置流水灯带和配套控制器安装，模拟食物从口腔、胃、小肠至大肠，灯光依次点亮，了解食物消化吸收的主要过程。","项",1]
[19,"洗手观察站","圆形灯箱","定制圆形超薄小灯箱，直径200-500mm以内，灯箱画面为正确洗手7步骤","个",7]
[20,"生命接力站","方形流线型灯箱","定制方形灯箱，内置15个分开控制灯组，对应灯箱画面，15个抢救步骤画面，可依次点亮对应抢救步骤灯箱","个",15]
[21,"医生训练营","心肺复苏模拟人半身","急救训练仿真模型 多功能教学模型 CPR心脏按压人工呼吸教学用模拟人全身 半身语音+LED灯指示","个",1]
[22,"展厅墙面","墙面新增磁吸展板","墙面磁吸板位置背板增加铁板和配套磁吸展板","块",30]
[23,"时光年轮区域","“时光年轮 ”处展台变化增加差价","1.定制烤漆展台，配套玻璃罩，内置积木台（展示物甲供），暂定尺寸L5900*H1170*W550mm（以二次深化为准）","个",1]
[24,"器械进化史","立式小展台","1.定制烤漆展台，配套玻璃罩，暂定尺寸L450*W400*H1300mm以内（详细尺寸二次深化为准）","个",10]
[25,null,"3D打印模型","1.定制医疗器械相关道具，旧物仿制或3D打印微缩模型，安装在展台玻璃罩内","组",10]

{"sheet":"计算式","index":1,"n_rows":73,"n_cols":22,"rows_kept":73,"hidden":true,"merged":[[0,0,0,5],[1,0,1,4],[3,1,3,4],[26,0,26,4],[27,1,27,4],[59,0,59,4],[60,1,60,4],[62,0,62,4],[63,0,63,4],[72,3,72,4],[73,3,73,4],[74,3,74,4]]}
["计算式"]
["工程名称：东宏股份智慧体验馆改造项目"]
["序号","项目名称","项目特征","单位","数量","汇总","EL-01","EL-02","EL-03","EL-04","EL-05","EL-06","EL-07","EL-08","EL-09","EL-10","EL-11","EL-12","EL-13","EL-14","EL-15","EL-16"]
["四","墙面"]
[1,"轻钢龙骨隔墙","1.100系轻钢龙骨，内置隔音棉                            2.横龙骨：U75*40*0.6mm 竖龙骨C75*50*0.6mm","m2",{"$f":"(338+242.7)*3.9","v":2264.73},{"$f":"SUM(G5:V5)","v":2322.57},{"$f":"(11.2+7.8+0.705*2)*4.2*2-7.2*3.5-6.5*2","v":{"v":133.244,"d":"133.24"}},{"$f":"(15.33-6.345+7.2+15.33+7.2)*4.2-13.46","v":149.143},{"$f":"(1.1+6+24)*4.2","v":130.62},{"$f":"(15.1-5.8+21.3-5.9)*4.2","v":103.74},{"$f":"(7.85+3.1+17.6)*4.2-7.17*3.3","v":96.249},{"$f":"(7.85+16.14+0.47*2+24)*4.2","v":205.506},{"$f":"(15.1+15.47)*4.2","v":128.394},{"$f":"(15.1+18.27)*4.2-7.2*3.3","v":116.394},{"$f":"(21.72+22.69-4.35)*4.2","v":168.252},{"$f":"(24.47+7+12.3)*4.2","v":183.834},{"$f":"(7+12.3-4.2+23.7-4.2)*4.2","v":145.32},{"$f":"(3.2+18.46+11.78)*4.2","v":140.448},{"$f":"(22.86+18.7)*4.2","v":174.552},{"$f":"(22.45+19.14)*4.2","v":174.678},{"$f":"(19.27+13.7)*4.2-6.6","v":131.874},{"$f":"(15.37+18.04)*4.2","v":140.322}]
[2,"造型木龙骨基础","1.木龙骨基础30*40，刷防火涂料","m2",{"$f":"(338+242.7)*3.9*0.4","v":{"v":905.892,"d":"905.89"}},153.433,{"$f":"5.8*2","v":11.6},{"$f":"13.3+5.7+1.4*4.1+(15.33+7.2)*4.1-15-14.04-14.02","v":74.053},26.26,{"$f":"10.3+9.4*4.1-21","v":27.84},{"$nulls":4},13.68]
[3,"基层板","1.12mm厚阻燃板基层2400*1200mm","m2",{"$f":"(338+242.7)*3.8","v":2206.66},2008.6575,{"$f":"(11.2+7.8+0.705*2)*4.1*2-7.2*3.5-6.5*2","v":{"v":129.162,"d":"129.16"}},{"$f":"(15.33-6.345+7.2+15.33+7.2)*4.1-13.46-15-14.04-14.02","v":102.2115},{"$f":"(1.1+6+24)*4.1","v":127.51},{"$f":"(15.1-5.8+21.3-5.9)*4.2","v":103.74},{"$f":"(7.85+3.1+17.6)*4.1-7.17*3.3","v":93.394},{"$f":"(7.85+16.14+0.47*2+24)*4.1-9.5-4.1-2.5-3.8-5.32","v":175.393},{"$f":"(7.4)*4.1","v":30.34},{"$f":"(15.1+18.27-7.7)*4.1-7.2*3.3","v":81.487},{"$f":"(21.72+22.69-4.35)*4.1","v":164.246},{"$f":"(24.47+7+12.3)*4.1-27.94","v":151.517},{"$f":"(7+12.3-4.2+23.7-4.2)*4.1","v":141.86},{"$f":"(3.2+18.46+11.78)*4.1-10.13","v":126.974},{"$f":"(22.86+18.7)*4.1","v":170.396},{"$f":"(22.45+19.14)*4.1","v":170.519},{"$f":"(19.27+13.7)*4.1-6.6-9-4.7","v":114.877},{"$f":"(15.37+18.04)*4.1-11.95","v":125.031}]
[null,"碳晶板","1.8mm碳晶板饰面，局部热弯弧度处理",null,null,1347.9296,{"$f":"(11.2+7.8+0.705*2)*4.1*2-7.2*3.5-6.5*2-6.2-13.5*2","v":{"v":95.962,"d":"95.96"}},{"$f":"H7-H9","v":28.6715},{"$f":"I7-I9","v":101.21},{"$f":"J7-J9","v":93.48},{"$f":"K7-10.4-20.8+3.14*1.1*0.65","v":64.4391},{"$f":"L7-21.72","v":153.673},null,null,{"$f":"O7-45.46","v":118.786},{"$f":"(24.47+7+12.3)*4.1-27.94-28.7-29.82","v":92.997},{"$f":"Q7-28.7","v":113.16},{"$f":"R7-R9","v":51.288},{"$f":"S7-S9-5.42-6.3*4.1","v":87.076},{"$f":"T7-T22-12.8-4.3","v":153.419},{"$f":"U7-U9","v":91.777},{"$f":"V7-V9-5.74","v":101.991}]
[4,"9.5mm厚石膏板","1.9.5mm厚石膏板2400*1200mm","m2",{"$f":"(338+242.7)*3.8*0.4","v":{"v":882.664,"d":"882.66"}},387.066,null,{"$f":"15+14.04+14.02+1.4*4.1+13.3+5.7+1.4*4.1","v":73.54},26.3,10.26,{"$f":"10.4-4.33+1.4*4.1","v":11.81},{"$f":"16.9-5.32+10.14","v":21.72},null,null,{"$f":"11.55+5.1+11.55+22.1-1.21*4","v":45.46},{"$f":"11.22+7.9+10.7","v":29.82},null,{"$f":"18.46*4.1","v":75.686},{"$f":"(6.1+5.2+1.4)*4.1","v":52.07},null,{"$f":"3.3*3.3+3.7*3.3","v":23.1},{"$f":"13.3+4","v":17.3}]
[null,"画面基层处理","1.板缝贴胶带、点锈，刮腻子三遍、画面基膜",null,null,387.066,null,{"$f":"15+14.04+14.02+1.4*4.1+13.3+5.7+1.4*4.1","v":73.54},26.3,10.26,{"$f":"10.4-4.33+1.4*4.1","v":11.81},{"$f":"16.9-5.32+10.14","v":21.72},null,null,{"$f":"11.55+5.1+11.55+22.1-1.21*4","v":45.46},{"$f":"11.22+7.9+10.7","v":29.82},null,{"$f":"18.46*4.1","v":75.686},{"$f":"(6.1+5.2+1.4)*4.1","v":52.07},null,{"$f":"3.3*3.3+3.7*3.3","v":23.1},{"$f":"13.3+4","v":17.3}]
[null,"12mm厚密度板","1.12mm密度板造型","m2",null,{"$f":"SUM(G11:V11)","v":57.4},{"$nulls":9},{"$f":"4.1*7","v":28.7},{"$f":"4.1*7","v":28.7}]
[null,"水性漆饰面","1.板缝贴胶带、点锈，刮腻子三遍、水性漆","m2",null,57.4,{"$nulls":9},{"$f":"4.1*7","v":28.7},{"$f":"4.1*7","v":28.7}]
[6,"新作玻璃饰面","1.12mm钢化玻璃新作","m2",{"$f":"17.2*3.75-20.89","v":43.61},22.96,null,{"$f":"1.4*4.1","v":5.74},null,null,{"$f":"1.4*4.1","v":5.74},{"$nulls":7},{"$f":"1.4*4.1","v":5.74},null,null,{"$f":"1.4*4.1","v":5.74}]
[null,"新作玻璃饰面","1.15mm超白玻璃","m2",{"v":0,"d":"0.00"},28.085,{"$nulls":11},{"$f":"0.55*4.1","v":2.255},{"$f":"6.3*4.1","v":25.83}]
[null,"玻璃隔板","1.15mm超白玻璃隔板W200mm","m",null,16.59,{"$nulls":3},{"$f":"2.765*6","v":16.59}]
[7,"不锈钢包边","1.12mm阻燃板基层，黑钛不锈钢包边W40mm内","m",{"v":91,"d":"91.00"},343.82,null,null,{"$f":"15.64+14.84+28.64+3.88","v":63},7,null,{"$f":"10.88+6.9+13.8+14.1","v":45.68},{"$f":"11.5+7.7+15.47*2","v":50.14},15.47,{"$f":"1.21*4","v":4.84},{"$f":"4.84*2+23.83","v":33.51},null,{"$f":"16.96+3.9","v":20.86},9.6,{"$f":"14.32+7+7.4+6.6","v":35.32},{"$f":"12.8+9.1","v":21.9},{"$f":"14.4+4.6+17.5","v":36.5}]
[8,"不锈钢造型包边","1.12mm阻燃板基层，黑钛不锈钢包边120mm以内","m",{"v":35,"d":"35.00"},61.07,null,{"$f":"16.94+16.14+16.06","v":49.14},4.7,7.23]
[null,"蓝色涂料边框","1.12mm阻燃板                                        2.9.5mm厚石膏板+蓝色涂料","m",null,23.8,null,{"$f":"14.1+9.7","v":23.8}]
[null,"圆形屏幕造型结构","1.钢木圆形框架","m2",null,27.91265,{"$nulls":3},{"$f":"3.14*1.15*1.15","v":{"v":4.15265,"d":"4.15"}},null,7.1,{"$nulls":3},1.8,null,null,14.86]
[9,"金属门套","1.12mm阻燃板                                        2.镜面不锈钢饰面","m2",{"$f":"(3.2+3*2)*0.62*2+(4.5+3*2)*0.24","v":{"v":13.928,"d":"13.93"}},66.2508,{"$nulls":4},{"$f":"(7.17*3.3*2)*1.4","v":66.2508}]
[null,"墙面吸音板",null,"m2",null,111.827,{"$nulls":6},{"$f":"(7.4)*4.1","v":30.34},{"$f":"(15.1+18.27-7.7)*4.1-7.2*3.3","v":81.487}]
[12,"墙面壁龛","1.内凹形墙面壁龛，亚克力透光背板，背发光，配套隔板","m2",{"$f":"5.5*2.7+1.9*2.7+1.5*1.12+0.58*0.8*6+15","v":{"v":39.444,"d":"39.44"}},34.888,{"$nulls":4},{"$f":"8*2.6","v":20.8},{"$f":"0.55*6+0.06*4+0.23+1.12*2","v":6.01},null,null,{"$f":"0.392*4+1.25+0.71+0.68+0.54+0.33","v":5.078},3]
[13,"金属饰面板包柱","1.镀锌角铁焊接圆形框架，不锈钢定制圆柱包柱","m2",{"$f":"2.66*3.8*2","v":{"v":20.216,"d":"20.22"}},33.4724,{"$nulls":4},{"$f":"3.14*1.3*4.1*2","v":{"v":33.4724,"d":"33.47"}}]
[14,"墙面灯槽","1.12mm阻燃板基层灯槽造型基层","m",{"$f":"3.9*8","v":{"v":31.2,"d":"31.20"}},913.55,{"$f":"9.2*2+1.2*11","v":31.6},10.76,11.26,{"$f":"13.3+14.75+22.04+6.8*2+6.1*2+6.85*2","v":89.59},{"$f":"15+21.22+2.7*4+0.15*6","v":47.92},{"$f":"19.32+10.1+3.7+9.7+7.5+6.8+13.3*2+14.22+17+16.02+9+12.8","v":152.76},{"$f":"3.5*9+1.4","v":32.9},{"$f":"28*3.5+0.8*4","v":101.2},{"$f":"17.68+10.38+17.68+30.38","v":76.12},{"$f":"17.28+13.28+16.68+1.94*3+23.7+4.1*2","v":84.96},{"$f":"4.1*2+10.4","v":18.6},null,{"$f":"38.76+18.6+10.76","v":68.12},{"$f":"13.64+4.61*2+4.83*2+3.6*2+12.1+8.5+16","v":76.32},{"$f":"15.1+10.3+8.1+10.6","v":44.1},{"$f":"2.6*6+1.6*24+13.34","v":67.34}]
[15,"暗门","1.800*2100mm 含五金                                2.30*30镀锌管骨架+12mm厚阻燃板基层+金属面板（暗门）\n3.背面9.5mm石膏板+喷白色无机涂料","樘",{"v":1,"d":"1.00"},3,1,{"$nulls":4},1,{"$nulls":5},1]
[16,"消火栓暗门（暂估）","1.700*1800mm                                 2.30*30镀锌管骨架+12mm厚阻燃板基层+4mm仿金属面铝塑板（暗门）\n3.背面9.5mm石膏板+喷白色无机涂料","樘",{"v":3,"d":"3.00"},5,5]
["小计"]
["六","美工展陈"]
[null,"墙面发光立体字/字母","1.定制亚克力激光雕刻发光字，H775mm","个",null,{"$f":"SUM(G29:V29)","v":8},8]
[null,"墙面发光立体字","1.定制亚克力激光雕刻发光字，H110-150mm","个",null,{"$f":"SUM(G30:V30)","v":90},null,5,{"$nulls":3},20,null,null,5,null,4,12,4,20,12,8]
[null,"墙面发光立体字","1.定制亚克力激光雕刻发光字，H180-200mm","个",null,{"$f":"SUM(G31:V31)","v":44},null,8,8,4,16,4,{"$nulls":7},4]
[null,"墙面立体字/字母","1.定制亚克力激光雕刻，H30-50mm","个",null,{"$f":"SUM(G32:V32)","v":913},null,32,null,null,32,{"$f":"55+11+112","v":178},null,null,{"$f":"59+40","v":99},{"$f":"116+38","v":154},{"$f":"25+40","v":65},null,32,20,{"$f":"73+170","v":243},{"$f":"32+26","v":58}]
[null,"墙面立体字/字母","1.定制亚克力激光雕刻，H50-100mm","个",null,{"$f":"SUM(G33:V33)","v":1679},null,{"$f":"22+17*2+60+16","v":132},{"$f":"68+27+18*4+19*8","v":319},25,106,{"$f":"107+156","v":263},null,null,{"$f":"18+6","v":24},15,14,74,113,{"$f":"95+86+19+43+27+80","v":350},{"$f":"27+71+75","v":173},{"$f":"32+24+15","v":71}]
[null,"墙面立体字/字母","1.定制亚克力激光雕刻，H100-200mm","个",null,236,null,20,{"$f":"16","v":16},4,null,{"$f":"26+12","v":38},null,null,13,25,6,62,8,24,16,4]
[null,"墙面立体字/字母","1.定制亚克力激光雕刻，H200-300mm","个",null,36,null,4,null,null,4,{"$nulls":7},{"$f":"20+4","v":24},null,null,4]
[3,"墙面画面","1.定制墙面画面","㎡",{"$f":"(6.4+7.1+3.8+7.2)*1.92+7*2.1+5.7*2.2+9.6*2+7.4*3.8+15.4*2","v":{"v":152.4,"d":"152.40"}},387.066,null,{"$f":"15+14.04+14.02+1.4*4.1+13.3+5.7+1.4*4.1","v":73.54},26.3,10.26,{"$f":"10.4-4.33+1.4*4.1","v":11.81},{"$f":"16.9-5.32+10.14","v":21.72},null,null,{"$f":"11.55+5.1+11.55+22.1-1.21*4","v":45.46},{"$f":"11.22+7.9+10.7","v":29.82},null,{"$f":"18.46*4.1","v":75.686},{"$f":"(6.1+5.2+1.4)*4.1","v":52.07},null,{"$f":"3.3*3.3+3.7*3.3","v":23.1},{"$f":"13.3+4","v":17.3}]
[null,"墙面即时贴文字","1.定制即时贴文字，<0.2㎡","套",null,33,null,null,10,{"$nulls":7},6,null,null,17]
[4,"附墙长形展台","1.定制烤漆展台，钢木结构骨架，烤漆饰面板，H650*W800mm","项（m）",{"v":1,"d":"1.00"},{"$f":"SUM(G38:V38)","v":19.5},{"$nulls":8},{"$f":"3.5*3+9","v":19.5}]
[null,"附墙地台","1.定制烤漆地台，钢木结构骨架，烤漆饰面板，H100*W1200mm","㎡",null,57.384,{"$nulls":8},{"$f":"(22.69+8.37)*1.2","v":37.272},{"$nulls":3},{"$f":"(16.76)*1.2","v":20.112}]
[null,"精品展柜","1.定制独脚支撑展柜，上置甲供零件，10mm钢化玻璃罩L605*W605*H820","个",null,6,{"$nulls":12},6]
[5,"长形插板模型台","1.定制烤漆模型展台，3400*1200mm，配套亚克力插板","个",{"v":1,"d":"1.00"},0]
[null,"长形展台","1.定制烤漆模型展台，L3000*W800*H800mm","个",{"v":1,"d":"1.00"},1,{"$nulls":13},1]
[6,"弧形展台","1.定制烤漆模型弧形展台","个",{"v":4,"d":"4.00"},{"$f":"SUM(G43:V43)","v":0}]
[7,"悬挑展台","1.定制钢结构烤漆悬挑台","项（m）",{"v":1,"d":"1.00"},5.6,{"$nulls":5},{"$f":"2.8*2","v":5.6}]
[null,"悬挑精品展台","1.定制墙面悬挑式精品展台，10mm钢化玻璃罩L1600*W830*H550mm","个",{"v":1,"d":"1.00"},3,{"$nulls":14},1,2]
[8,"沙盘台","1.定制烤漆沙盘展台，7200*6400mm","个",{"v":1,"d":"1.00"},0]
[9,"沙盘模型","1.定制模型沙盘","㎡",{"$f":"2.7*2.4+2.7*3.6+3.3*3.5","v":27.75},0]
[null,"亚克力线条",null,"m",null,{"$f":"SUM(G48:V48)","v":94.99},{"$nulls":8},{"$f":"9+9.8+14.4+15.25+2.42","v":50.87},{"$f":"16.45+15.28+3.59+8.8","v":44.12}]
[null,"造型透明管","1.亚克力/玻璃透明圆管，内置跑马灯","m",null,69.82,{"$nulls":9},{"$f":"2.4+1.5*2+2.76*2","v":10.92},null,{"$f":"12.3*2+16+15+3.3","v":58.9}]
[null,"深渊镜","1.LED灯带、单透镜、镜面玻璃定制深渊镜，含配套结构","㎡",null,18.45,{"$nulls":11},{"$f":"3.2*4.1","v":13.12},{"$nulls":3},5.33]
[10,"墙面展板","1.墙面雪弗板/亚克力UV展板","项",{"v":1,"d":"1.00"},151,null,{"$f":"4+6","v":10},20,null,null,{"$f":"9+18","v":27},null,null,6,{"$f":"2+7","v":9},{"$f":"10+7","v":17},null,{"$f":"9+17","v":26},13,{"$f":"6+13","v":19},4]
[11,"奖牌复刻","1.奖牌复刻","项",{"v":1,"d":"1.00"},0]
[12,"磁吸展板","1.墙面定制磁吸展板","项",{"v":1,"d":"1.00"},0]
[13,"墙面灯箱","1.定制墙面软膜/亚克力灯箱","项",{"v":1,"d":"1.00"},52.631,null,null,{"$f":"13.2+11.3*0.07","v":13.991},2.3,{"$nulls":9},{"$f":"4.9*3.5*2+0.8","v":35.1},null,1.24]
[14,"造型“树”形装置","1.定制造型树装置","项",{"v":1,"d":"1.00"},0]
[15,"墙面雕刻板","1.墙面定制造型雕刻板","项",{"v":1,"d":"1.00"},16.55,null,2.45,{"$nulls":10},14.1]
[16,"墙面物理互动装置","1.旋转装置，不同位置灯箱点亮","项",{"v":1,"d":"1.00"},1,{"$nulls":3},1]
[17,"造型门","1.W2400mm，定制圆弧形造型仿太空舱门门套，模型开模浇筑，玻璃钢打磨喷漆，2樘","项",{"v":1,"d":"1.00"},1]
[19,"地贴","1.定制地贴","项",{"v":1,"d":"1.00"},1]
["小计"]
["七","其他"]
[1,"脚手架","1.脚手架租赁","m2",{"$f":"2135.7-73.3-156.2-45.7","v":{"v":1860.5,"d":"1860.50"}}]
["小计"]
["建安工程费合计"]
[1,"安全文明施工及临时设施费",{"v":0.03,"d":"3.00%"},"项",{"v":1,"d":"1.00"},"现场安全围挡、二次搬运等措施费用"]
[2,"管理费",{"v":0.05,"d":"5.00%"},"项",{"v":1,"d":"1.00"}]
[null,"未税合计"]
[1,"税金",{"v":0.09,"d":"9.00%"},"项",{"v":1,"d":"1.00"}]
[null,"工程费用总计"]
[]
[]
[]
[{"$nulls":3},{"$f":"#REF!/E62","v":{"$error":"#REF!"}}]